[V1.6]
-Change layout: Separate device info to an individual text field.
-Add "Cascade" version for VMR7100+VMC6210 product.

---------------

[V1.5]
-Change: Save embedded EzAux log with current boot section by default.
-Fine tune in RC set/get commands.
-Fix: All buttons will be grayed out if unplug device when updating.

---------------

[V1.4]
-Add save embedded EzAux log function.

---------------

[V1.3]
-Remove VID/PID block, now will find Spyder/Carrera device automatically when clicked Open button.
-Add device remove callback, Close button will be triggered when current opening device is removed.

Known issues and check list:
-Only support Spyder and Carrera, EzAux R2 will supported in future version.

---------------

[V1.2]
-Fix for Carrera support.

---------------

[V1.1]
-Add dump register and memory function.
-Fix log content in update firmware.
-Show firmware name when device opened.
-Add device type checking(only support Spyder and Carrera).

Known issues and check list:
-Only support Spyder and Carrera(Carrera is not tested yet).
-Show target firmware version(read version from FW file)?
-Not handling device removed message, user should click open/close device manually.

---------------

[V1.0]
-First release.

Known issues and check list:
-Only support Spyder device. Not check device type yet.
-Show target firmware version(read version from FW file)?
-Not handling device removed message, user should click open/close device manually.
-Add dump function?
